Altium Designer Pick and Place Locations
C:\ownCloud\Prace\VlastniDPS\timekeeping_hw\HW_LaserSensor\Dokumentace\v0.1\Pick&Place\pick&place_timeKeeping_LaserSensor_v0.1_2019-12-15_default_PetrVitek.txt

========================================================================================================================
File Design Information:

Date:       15.12.19
Time:       15:02
Revision:   Not in VersionControl
Variant:    default
Units used: mm

Designator Comment               Layer    Footprint Center-X(mm) Center-Y(mm) Rotation name               Value          
C1         UniversalCapacitor    TopLayer C0402     4.2000       4.0630       90       0402B104K250CT     "100nF 25V"    
C2         4.7uF/10V             TopLayer C0402_big 5.3000       4.0630       270      GRM155R61A475MEAAD 4.7uF/10V      
D1         ZenerDiode            TopLayer SOD523    2.7750       3.9750       270      PESD3V3S1UB        ""             
D2         RClamp0524PA          TopLayer SLP2510P8 7.6250       4.0630       90       RCLAMP0524PATCT    RCLAMP0524PA   
IC1        VL53L1X               TopLayer VL53L1X   6.5000       7.2750       180      VL53L1CXV0FY/1     VL53L1CXV0FY/1 
R1         UniversalResistor0402 TopLayer R0402     10.0029      4.0630       90       CRCW04024K70FKED   4K7-1%         
